ANNEX

**Amendments to Annex IV to Regulation (EU) No 168/2013**

In Annex IV to Regulation (EU) No 168/2013, the table is amended as follows:

* + - 1. points 1.1.2.1., 1.1.2.2. and 1.1.2.3. are replaced by the following:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ‘1.1.2.1. | Euro 4: Annex VI A1 | L1e, L2e, L6e | 1.1.2017 | 1.1.2018 | 31.12.2020; for L2e-U and L6e-B: 31.12.2022 |
| 1.1.2.2. | Euro 4: Annex VI A1 | L3e,L4e,L5e,L7e | 1.1.2016 | 1.1.2017 | 31.12.2020; for L3e-AxE and L3e-AxT 31.12.2022 |
| 1.1.2.3. | Euro 5: Annex VI A2 | L1e-L7e | 1.1.2020;for L2e-U; L3e-AxE ;L3e-AxT and L6e-B: 1.1.2022 | 1.1.2021;for L2e-U; L3e-AxE; L3e-AxT and L6e-B: 1.1.2023 | ’; |

* + - 1. points 1.8.1., 1.8.2. and 1.8.3. are replaced by the following:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ‘1.8.1. | OBD stage I functional requirements | L3e, L4e, L5e-A, L7e-A | 1.1.2016 | 1.1.2017 | 31.12.2020 |
| OBD stage I environmental test procedure (test type VIII) |
| OBD stage I environmental test thresholds, Annex VI (B1) |
| 1.8.2. | OBD stage I functional requirements including any operating mode which significantly reduces engine torque | L3e, L4e,L5e,L7e | 1.1.2020 | 1.1.2021 | 31.12.2024 |
| OBD stage I environmental test procedure (test type VIII) |
| OBD stage I environmental test thresholds, Annex VI (B1) |
| 1.8.3. | OBD stage I functional requirements including any operating mode which significantly reduces engine torque | L3e, L4e,L5e,L7e | 1.1.2024 | 1.1.2025 | ’; |
| OBD stage I environmental test procedure (test type VIII) |
| OBD stage I environmental test thresholds, Annex VI (B2) |

* + - 1. the following points are inserted:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ‘1.8.4. | OBD stage II functional requirementswith the exception of catalyst monitoring | L3e, L4e,L5e-A, L7e-A | 1.1.2020 | 1.1.2021 | 31.12.2024 |
| OBD stage II environmental test procedures (test type VIII) |
| OBD stage II environmental test thresholds, Annex VI (B1 |
| 1.8.5. | OBD stage II functional requirements,  | L3e, L4e, L5e‑A, L7e-A | 1.1.2024 | 1.1.2025 | ’; |
| OBD stage II environmental test procedures (test type VIII),  |
| OBD stage II environmental test thresholds, Annex VI (B2) |

* + - 1. points 1.9.1. and 1.9.2. are replaced by the following:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ‘1.9.1. | Sound level test procedure and limit values Annex VI (D) | L1e, L2e, L6e | 1.1.2017 | 1.1.2018 |  |
| 1.9.2. | Sound level test procedure and limit values (3), Annex VI (D) | L3e, L4e, L5e, L7e | 1.1.2016 | 1.1.2017 | ’; |

* + - 1. point 1.9.4. is replaced by the following:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ‘1.9.4. | UNECE regulations Nos 9, 41, 63, 92 and associated new limit values proposed by the Commission | L1e-L7e |  |  | ’. |