ANNEX

In Annex I to Regulation (EC) No 715/2007, the following Table 2a is inserted:

“*Table 2a*

**Real Driving Emissions Conformity Factors**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | Oxides of nitrogen (NOx) | Number of particles (PN) | Carbon monoxide (CO)([[1]](#footnote-1)) | Total hydrocarbons (THC) | Combined hydrocarbons and oxides of nitrogen (THC + NOx) |
| *CFpollutant-final (2)* | 1,43 | 1,5 | - | - | - |
| *CF pollutant-temp*(3) | 2,1 | 1,5 | - | - | - |

(1) CO emissions shall be measured and recorded for all RDE tests.

 (2) *CFpollutant-final* is the conformity factor used to determine compliance with the Euro 6 emission limits by taking into account the technical uncertainties linked with the use of the Portable Emission Measurement Systems (PEMS).

 (3) CF *pollutant-temp* is the temporary conformity factor that may be used upon request of the manufacturer as an alternative to *CFpollutant-final* during a period of 5 years and 4 months following the dates specified in Article 10(4) and (5).”.

1. [↑](#footnote-ref-1)