

CORRIGENDUM

to Commission Delegated Regulation (EU) No C(2015)4394 final of 1 July 2015 on the classification of the reaction to fire performance of construction products pursuant to Regulation (EU) No 305/2011 of the European Parliament and of the Council

(Text with EEA relevance)

In Section 1.3 of Annex to the Regulation, line (3) has to be deleted and the numbering adjusted accordingly.

In Annex to the Regulation, within Table 3, the boxes in the rows for classes A1**L** and A2**L** of the third column (“Classification criteria”) have to be corrected as below:

*for:* 'T' and ‘m’

*read:* 'ΔT' and ‘Δm’.