ANNEX

In Part A of Annex III to Directive 2004/37/EC, the following entries are added:

| **CAS No** ([[1]](#footnote-1)) | **EC No** ([[2]](#footnote-2)) | **NAME OF AGENT** | **LIMIT VALUES** | **TRANSITIONAL MEASURES** |
| --- | --- | --- | --- | --- |
| **8 hours** ([[3]](#footnote-3)) | **Short-term** ([[4]](#footnote-4)) |  |
| **mg/m3** ([[5]](#footnote-5)) | **ppm** ([[6]](#footnote-6)) | **f/ml**([[7]](#footnote-7)) | **mg/m3** | **ppm** | **f/ml** |  |
| 79-01-6 | 201-167-4 | Trichloroethylene | 54,7 | 10 | \_ | 164,1 | 30 | \_ |  |
| 101-77-9 | 202-974-4 | 4,4'-Methylenedianiline | 0,08 | \_ | ­\_ | \_ | \_ | \_ |  |
| 106-89-8 | 203-439-8 | Epichlorohydrine | 1,9  | \_ | ­\_ | \_ | \_ | \_ |  |
| 106-93-4 | 203-444-5 | Ethylene dibromide | 0,8  | 0,1 | \_ | \_ | \_ | \_ |  |
| 107-06-2 | 203-458-1 | Ethylene dichloride | 8,2  | 2 | \_ | ­­\_ | \_ | \_ |  |

The Column "Notation" in Part A of Annex III to Directive 2004/37/EC and the notations set out in that column are transferred to Part B of Annex III to Directive 2004/37/EC.

In Part B of Annex III to Directive 2004/37/EC, the following entries are added:

| **CAS No** ([[8]](#footnote-8)) | **EC No** ([[9]](#footnote-9)) | **NAME OF AGENT** | **Notation**([[10]](#footnote-10)) |
| --- | --- | --- | --- |
|
| \_ | \_ | Polycyclic aromatic hydrocarbons mixtures containing benzo[*a*]pyrene which are carcinogens within the meaning of the Directive | skin  |
| \_ | \_ | Oils that have been used before in internal combustion engines to lubricate and cool the moving parts within the engine | skin |
| 71-43-2 | 200-753-7 | Benzene  | skin |
| 79-01-6 | 201-167-4 | Trichloroethylene | skin |
| 101-77-9 | 202-974-4 | 4,4'-Methylenedianiline | skin |
| 106-89-8 | 203-439-8 | Epichlorohydrine | skin |
| 106-93-4 | 203-444-5 | Ethylene dibromide | skin |
| 107-06-2 | 203-458-1 | Ethylene dichloride | skin |

1. CAS No: Chemical Abstract Service Registry Number. [↑](#footnote-ref-1)
2. EC No, i.e. EINECS, ELINCS or NLP, is the official number of the substance within the European Union, as defined in section 1.1.1.2 in Annex VI, Part 1, of Regulation (EC) No 1272/2008. [↑](#footnote-ref-2)
3. Measured or calculated in relation to a reference period of eight hours time-weighted average (TWA). [↑](#footnote-ref-3)
4. Short-term exposure limit (STEL). A limit value above which exposure should not occur and which is related to a 15-minute period unless otherwise specified. [↑](#footnote-ref-4)
5. mg/m3 = milligrams per cubic metre of air at 20°C and 101,3 kPa (760 mm mercury pressure). [↑](#footnote-ref-5)
6. ppm = parts per million by volume in air (ml/m3). [↑](#footnote-ref-6)
7. f/ml = fibres per millilitre. [↑](#footnote-ref-7)
8. CAS No: Chemical Abstract Service Registry Number. [↑](#footnote-ref-8)
9. EC No, i.e. EINECS, ELINCS or NLP, is the official number of the substance within the European Union, as defined in section 1.1.1.2 in Annex VI, Part 1, of Regulation (EC) No 1272/2008. [↑](#footnote-ref-9)
10. Substantial contribution to the total body burden via dermal exposure possible. [↑](#footnote-ref-10)